; This is the configuration for the 'pypad_nautel.py' script for
; Rivendell, which can be used to output Now & Next data to one or more
; Nautel VS transmitters as RDP in ASCII TCP mode.

; Section Header
;
[Rds1]

; *****************************************************************************
; TCP/IP Connection Settings
;  IP Address
;
; The IP address of the TCP port to send updates to, in dotted-quad notation.
; If using a serial connection, leave this entry blank!
IpAddress=127.0.0.1

; TCP Port
;
; The TCP port number to send updates to, in the range 0 - 65,535.  
TcpPort=7005

; *****************************************************************************

; Output Strings.  The PAD data to output each time RDAirPlay changes
; play state, including any wildcards as placeholders for metadata values.
;
; For the list of supported wildcards. see the 'Metadata Wildcards' section
; of the Rivendell Operations Guide.
;
; I recommend setting just these three unless you really know what you're doing
; documentation is in section 2 of the VS OPS Manual.  
; In issue 10.0 for the NV2.5 this is on page 2-69

;Program Service - 8 character ASCII tagline, often callsign or a short name
ProgramService=
;Dynamic PS - 
DynamicPS=%t - %a
;Radio Text - up to 64 characters
RadioText=%t - %a

;; These settings are not recommended to be changed unless you really know
;; what you are doing and why you are doing it.  
;; Per the manual, not all values can be unset by the TCP ASCII connection.
;;PICode= ***SET THIS IN YOUR TRANSMITTER PER THE RDS/RDBS SPEC***
;ProgramType=0
;ProgramTypeName=
;TrafficProgram=0
;TrafficAnnouncement=0
;AltFreq1=107
;AltFreq2=107
;AltFreq3=107
;AltFreq4=107
;AltFreq5=107
;AltFreq6=107
;AltFreq7=107
;AltFreq8=107
;AltFreq9=107
;AltFreq10=107
;AltFreq11=107
;AltFreq12=107
;AltFreq13=107
;AltFreq14=107
;AltFreq15=107
;AltFreq16=107
;AltFreq17=107
;AltFreq18=107
;AltFreq19=107
;AltFreq20=107
;AltFreq21=107
;AltFreq22=107
;AltFreq23=107
;AltFreq24=107
;AltFreq25=107
;DecoderInfo=3
;MusicSpeech=1
;Date=
;Time=
;UTCOffset=39
;Cont=
;DPSRate=0
;DPSMode=0



; Log Selection
;
; Set the status for each log to 'Yes', 'No' or 'Onair' to indicate whether
; state changes on that log should be output on this udp port.  If set
; to 'Onair', then output will be generated only if RDAirPlays OnAir flag
; is active.
MasterLog=Yes
Aux1Log=Yes
Aux2Log=Yes
VLog101=No
VLog102=No
VLog103=No
VLog104=No
VLog105=No
VLog106=No
VLog107=No
VLog108=No
VLog109=No
VLog110=No
VLog111=No
VLog112=No
VLog113=No
VLog114=No
VLog115=No
VLog116=No
VLog117=No
VLog118=No
VLog119=No
VLog120=No


[NowGroups]
; Group Selection
;
; Filter updates according to the Group membership of the 'now' playing
; event. If no groups are listed here and in the [NextGroups] section,
; then ALL updates will be forwarded
; without regard to Group.
; Group1=MUSIC
; Group2=LEGAL
; [...] ; Additional groups can be added...

[NextGroups]
; Group Selection
;
; Filter updates according to the Group membership of the 'next' playing
; event. If no groups are listed here, If no groups are listed here and in
; the [NowGroups] section,then ALL updates will be forwarded
; without regard to Group.
; Group1=MUSIC
; Group2=LEGAL
; [...] ; Additional groups can be added...
