; This is the sample configuration for the 'pypad_shoutcast1.py' script for 
; Rivendell, which can be used to update the metadata on a Shoutcast
; server using Now & Next data.


; Section Header
;
; One section per Shoutcast server instance is configured, starting with 
; 'Shoutcast1' and working up consecutively
[Shoutcast1]

; Username
;
; The username for the Shoutcast server instance to which to send updates.
; (This option is seldom required).
Username=

; Password
;
; The password of the Shoutcast server instance to which to send updates.
Password=changeme

; Host Name
;
; The fully-qualified domain name or IP address of the Shoutcast server
Hostname=shoutcast.example.com

; Host Port
;
; The TCP port number of the Shoutcast server
Tcpport=8000

; Format String.  The metadata to be sent each time RDAirPlay changes
; play state, including any wildcards as placeholders for metadata values.
;
; The list of available wildcards can be found in the 'metadata_wildcards.txt'
; file in the Rivendell documentation directory.
;
FormatString=%a - %t

; Log Selection
;
; Set the status for each log to 'Yes', 'No' or 'Onair' to indicate whether
; state changes on that log should be output to this account.  If set
; to 'Onair', then output will be generated only if RDAirPlays OnAir flag
; is active.
MasterLog=Yes
Aux1Log=Yes
Aux2Log=Yes
VLog101=No
VLog102=No
VLog103=No
VLog104=No
VLog105=No
VLog106=No
VLog107=No
VLog108=No
VLog109=No
VLog110=No
VLog111=No
VLog112=No
VLog113=No
VLog114=No
VLog115=No
VLog116=No
VLog117=No
VLog118=No
VLog119=No
VLog120=No


; Additional Shoutcast server instances can be configured by adding new
; sections...
;
;[Shoutcast2]
;Password=letmein
;Hostname=anotherone.example.com
;Tcpport=80
;FormatString=%t by %a
;MasterLog=Yes
;Aux1Log=No
;Aux2Log=Onair
;VLog101=No
;VLog102=No
;VLog103=No
;VLog104=No
;VLog105=No
;VLog106=No
;VLog107=No
;VLog108=No
;VLog109=No
;VLog110=No
;VLog111=No
;VLog112=No
;VLog113=No
;VLog114=No
;VLog115=No
;VLog116=No
;VLog117=No
;VLog118=No
;VLog119=No
;VLog120=No
