; This is the configuration for the 'pypad_liqcomp.py' module for 
; Rivendell, which can be used to output Now & Next data to one or more
; Liquid Compass Internet streaming encoders, using the following format:
;
; |<title>|<artist>|<cart-num>|<length>|<group>|<album>|<label>|<lf>

; Section Header
;
; One section per remote encoder is configured, starting with 'System1' and 
; working up consecutively
[System1]

; IP Address
;
; The IP address of the remote encoder, in dotted-quad notation.
IpAddress=192.168.10.22

; UDP Port
;
; The UDP port number of the remote encoder, in the range 0 - 65,535.
UdpPort=5273

; Field Definitions.  The string to use to populate the <title>, <artist>,
; <album> and <label> fields sent to ANDO each time RDAirPlay changes play
; state.   These can include wildcards as placeholders for metadata values.
; For the list of supported wildcards. see the 'Metadata Wildcards' section
; of the Rivendell Operations Guide.
Title=%t
Artist=%a
Album=%l
Label=%b

; Log Selection
;
; Set the status for each log to 'Yes', 'No' or 'Onair' to indicate whether
; state changes on that log should be output on this udp port.  If set
; to 'Onair', then output will be generated only if the RDAirPlay OnAir flag
; is active.
MasterLog=Yes
Aux1Log=Yes
Aux2Log=Yes
VLog101=No
VLog102=No
VLog103=No
VLog104=No
VLog105=No
VLog106=No
VLog107=No
VLog108=No
VLog109=No
VLog110=No
VLog111=No
VLog112=No
VLog113=No
VLog114=No
VLog115=No
VLog116=No
VLog117=No
VLog118=No
VLog119=No
VLog120=No


; Additional encoders can be configured by adding new sections...
;[System2]
;IpAddress=192.168.10.22
;UdpPort=6789
;Title=%u
;Artist=%a
;Album=%p
;MasterLog=Yes
;Aux1Log=No
;Aux2Log=Onair
;VLog101=No
;VLog102=No
;VLog103=No
;VLog104=No
;VLog105=No
;VLog106=No
;VLog107=No
;VLog108=No
;VLog109=No
;VLog110=No
;VLog111=No
;VLog112=No
;VLog113=No
;VLog114=No
;VLog115=No
;VLog116=No
;VLog117=No
;VLog118=No
;VLog119=No
;VLog120=No
