; This is the configuration for the 'pypad_serial.py' script for
; Rivendell, which can be used to output Now & Next data via one or more
; serial ports.
;
; NOTE: The serial ports configured here have NOTHING TO DO with the
;       ports configured in RDAdmin! These ports are used strictly by the
;       'pypad_serial.py' plugin, and will not be usable by any other Rivendell
;       component.

; Section Header
;
; One per serial device to be configured, starting with 'Serial1' and
; working up consecutively
[Serial1]

; Serial Device
;
; The device file that corresponds to the serial device.
Device=/dev/ttyS0

; Serial Baud Rate (in bps)
Speed=9600

; Parity (0=none, 1=even, 2=odd)
Parity=0

; Number of bits per data 'word'.
WordSize=8

; Format String.  The string to be output each time RDAirPlay changes
; play state, including any wildcards as placeholders for metadata values.
;
; The list of available wildcards can be found in the 'metadata_wildcards.txt'
; file in the Rivendell documentation directory.
;
FormatString=NOW: %d(ddd MMM d hh:mm:ss yyyy): %t - %a\r\nNEXT: %D(ddd MMM d hh:mm:ss yyyy): %T - %A\r\n

; Encoding.  Defines the set of escapes to be applied to the PAD fields.
; The following options are available:
;
;  0 - Perform no character escaping.
;  1 - "XML" escaping: Escape reserved characters as per XML-v1.0
;  2 - "Web" escaping: Escape reserved characters as per RFC 2396 Section 2.4
Encoding=0

; Null Update Handling.  Defines how 'null' updates --i.e. those with a cart
; number of '0' -- should be handled.
;
;  0 - Process all updates regardless of cart values.
;  1 - Process update only if the 'now' cart is not null.
;  2 - Process update only if the 'next' cart is not null.
;  3 - Process update only if both the 'now' and 'next' carts are not null.
ProcessNullUpdates=0

; Log Selection
;
; Set the status for each log to 'Yes', 'No' or 'Onair' to indicate whether
; state changes on that log should be output on this serial port.  If set
; to 'Onair', then output will be generated only if RDAirPlay's OnAir flag
; is active.
MasterLog=Yes
Aux1Log=Yes
Aux2Log=Yes
VLog101=No
VLog102=No
VLog103=No
VLog104=No
VLog105=No
VLog106=No
VLog107=No
VLog108=No
VLog109=No
VLog110=No
VLog111=No
VLog112=No
VLog113=No
VLog114=No
VLog115=No
VLog116=No
VLog117=No
VLog118=No
VLog119=No
VLog120=No


; Additional serial ports can be configured by adding new sections...
;[Serial2]
;Device=/dev/ttyS1
;Speed=9600
;Parity=0
;WordSize=8
;FormatString=%t
;ProcessNullUpdates=0
;MasterLog=Yes
;Aux1Log=No
;Aux2Log=Onair
;VLog101=No
;VLog102=No
;VLog103=No
;VLog104=No
;VLog105=No
;VLog106=No
;VLog107=No
;VLog108=No
;VLog109=No
;VLog110=No
;VLog111=No
;VLog112=No
;VLog113=No
;VLog114=No
;VLog115=No
;VLog116=No
;VLog117=No
;VLog118=No
;VLog119=No
;VLog120=No
